**Supplementary Information**

**Distributions and risks of SARS-CoV-2 in hospital outdoor environment**

Dayi Zhang1,\*, Yunfeng Yang1, Xia Huang1, Jingkun Jiang1, Miao Li1, Xian Zhang1, Haibo Ling2, Jing Li3, Yi Liu1, Guanghe Li1, Weiwei Li2, Chuan Yi2, Ting Zhang3, Yongzhong Jiang3, Songqiang Deng4, Peng Zhao4, Jiuhui Qu1,5,\*

1. School of Environment, Tsinghua University, Beijing 100084, P.R. China
2. Hubei Academy of Environmental Sciences, Wuhan 430072, P.R. China
3. Hubei Center for Disease Control and Prevention, Wuhan 430079, P.R. China
4. Research Institute for Environmental Innovation (Tsinghua-Suzhou), Suzhou 215163, P.R. China
5. Key Laboratory of Drinking Water Science and Technology, Research Center for Eco-Environmental Sciences, Chinese Academy of Sciences, Beijing 100085, P.R. China

**Corresponding author**

Dr Dayi Zhang

School of Environment, Tsinghua University, Beijing 100084, P.R. China

Email: zhangdayi@tsinghua.edu.cn

Tel: +86(0)10-62773232; Fax: +86(0)10-62795687

Prof Jiuhui Qu

School of Environment, Tsinghua University, Beijing 100084, P.R. China

Email: jhqu@tsinghua.edu.cn

Tel: +86(0)10-62849151; Fax: +86(0)10-62795687



(A)



(B)



(C)

**Figure S1.** Schematic medical wastewater treatment sectors in Jinyintan Hospital (A), Huoshenshan Hospital (B) and Wuchang Fangcang Hospital (C).

**Table S1.** Copy numbers of SARS-CoV-2 viral RNA in each sampling points of hospital outdoor environment.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Hospital** | **Sampling sites** | **Samples** | **Description** | **SARS-CoV-2** |
| **Jinyintan** | **Wastewater treatment sector** | **Water** | **Adjusting tank** | **255 copies/L** |
| Water | Aeration tank | ND |
| Water | Secondary sedimentation tank | ND |
| Water | Disinfection tank | ND |
| Water | Effluent | ND |
| **Aerosol** | **Inside adjusting tank** | **285 copies/m3** |
| **Soil** | **2 m away from the adjusting tank** | **253 copies/g** |
| Soil | 2 m away from the disinfection tank | ND |
| **Out- and In-patient department** | **Aerosol** | **5 m away from outpatient department** | **1130 copies/m3** |
| Aerosol | 5 m away from inpatient department | ND |
| Soil | 20 m away from outpatient department | ND |
| **Soil** | **10 m away from inpatient department** | **205 copies/g** |
| Surface | Road surface 5 m away from outpatient department | ND |
| Surface | Road surface 5 m away from inpatient department | ND |
| **Background** | Aerosol | 100 m away from inpatient department | ND |
| Soil | 100 m away from inpatient department | ND |
| Surface | Road surface 100 m away from inpatient department | ND |
| **Huoshenshan** | **Wastewater treatment sector** | **Water** | **First adjusting tank** | **633 copies/L** |
| Water | Septic tank | ND |
| Water | Second adjusting tank | ND |
| **Water** | **MBBR** | **ND-505 copies/L** |
| **Water** | **Sedimentation tank** | **ND-2.2×103 copies/L** |
| Water | Effluent after disinfection | ND |
| **Aerosol** | **Inside septic tank** | **603 copies/m3** |
| Aerosol | Inside third adjusting tank | ND |
| **Soil** | **2 m away from first adjusting tank** | **550 copies/g** |
| Soil | 2 m away from second adjusting tank | ND |
| Surface | MBBR outside wall | ND |
| Surface | Road surface 2 m away from MBBR | ND |
| **Background** | Aerosol | Medical staff living area | ND |
| Soil | Medical staff living area | ND |
| Surface | Medical staff living area | ND |
| **Wuchang Fangcang** | **Wastewater treatment sector** | Water | Preliminary disinfection tank | ND |
| **Water** | **Septic tank\*** | **557 to 1.9×104 copies/L** |
| Water | Septic tank\*\* | ND |
| Aerosol | 2 m away from the septic tank | ND |
| Soil | 2 m away from the septic tanks | ND |
| Surface | Road surface 10 m away from the septic tank | ND |
| **Entrance** | Aerosol | 5 m away from the entrance | ND |
| Surface | Steps of the entrance | ND |
| Surface | Road surface 5 m away from the entrance | ND |
| **Outdoor toilet** | Aerosol | Outdoor toilet | ND |
| Surface | Ground of outdoor toilets | ND |
| Surface | Outside wall of outdoor toilets | ND |
| Surface | Road surface 5 m away from outdoor toilets | ND |
| **Background** | Aerosol | 100 m away from hospital | ND |
| Soil | 100 m away from hospital | ND |
| Surface | Road surface 100 m away from hospital) | ND |

ND, non-detected.

\* Before 5th March and \*\* after 5th March.