**Dental mitigation strategies to reduce aerosolization of SARS-CoV-2**

Jon J. Vernon 1, Emma V. I. Black 1, Thomas Dennis 2, Deirdre A. Devine 1, Louise Fletcher 3, David J Wood 1, Brian R Nattress 4\*

 1. Division of Oral Biology, School of Dentistry, University of Leeds, UK

 2. Leeds Dental Institute, Leeds Teaching Hospitals Trust, Leeds, UK

 3. School of Civil Engineering, University of Leeds, Leeds, UK

 4. Division of Restorative Dentistry, School of Dentistry, University of Leeds, UK

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| UL2 – Dentist Position |  | 0.3 µm | 0.5 µm | 1.0 µm | 3.0 µm | 5.0 µm | 10.0 µm |
| Air Turbine | No mitigation | Mean | 6.54E+06 | 1.97E+06 | 6.14E+05 | 6.04E+04 | 3.06E+04 | 1.66E+04 |
| ± STD Error | 1.31E+06 | 4.03E+05 | 1.31E+05 | 2.13E+04 | 1.23E+04 | 6.71E+03 |
| High-Volume Aspiration | Mean | 1.66E+06 | 4.36E+05 | 9.59E+04 | 8.14E+03 | 4.74E+03 | 2.72E+03 |
| ± STD Error | 2.88E+05 | 5.33E+04 | 4.36E+02 | 2.33E+02 | 7.57E+01 | 2.52E+01 |
| Dam | Mean | 1.12E+06 | 4.84E+05 | 1.53E+05 | 2.31E+04 | 1.08E+04 | 5.26E+03 |
| ± STD Error | 9.15E+05 | 2.22E+05 | 6.32E+04 | 8.07E+03 | 4.74E+03 | 2.40E+03 |
| Aerosol Extraction Device | Mean | 7.61E+06 | 1.28E+06 | 2.42E+05 | 3.94E+04 | 1.88E+04 | 9.01E+03 |
| ± STD Error | 1.95E+05 | 6.59E+03 | 0.00E+00 | 1.34E+03 | 8.17E+02 | 1.40E+02 |
| Electric Rotor | No mitigation | Mean | 5.73E+05 | 1.44E+05 | 7.36E+02 | 7.73E+02 | 1.77E+02 | 5.88E+01 |
| ± STD Error | 7.04E+05 | 1.95E+05 | 8.55E+04 | 1.49E+04 | 6.45E+03 | 3.05E+03 |
| High-Volume Aspiration | Mean | 2.01E+05 | 6.59E+03 | 0.00E+00 | 1.34E+03 | 8.17E+02 | 1.40E+02 |
| ± STD Error | 1.14E+06 | 7.09E+04 | 1.99E+03 | 0.00E+00 | 0.00E+00 | 0.00E+00 |
| Dam | Mean | 1.90E+06 | 9.55E+04 | 2.80E+03 | 0.00E+00 | 0.00E+00 | 0.00E+00 |
| ± STD Error | 3.32E+06 | 3.88E+05 | 2.44E+04 | 3.83E+03 | 2.38E+03 | 1.48E+03 |
|  |  |  |  |  |  |  |  |  |
| UL2 – Door Position |  | 0.3 µm | 0.5 µm | 1.0 µm | 3.0 µm | 5.0 µm | 10.0 µm |
| Air Turbine | No mitigation | Mean | 6.63E+06 | 1.96E+06 | 5.86E+05 | 4.59E+04 | 2.30E+04 | 1.12E+04 |
| ± STD Error | 1.05E+06 | 2.57E+05 | 7.58E+04 | 1.01E+04 | 5.59E+03 | 2.76E+03 |
| High-Volume Aspiration | Mean | 1.70E+06 | 4.14E+05 | 8.37E+04 | 5.66E+03 | 2.17E+03 | 8.48E+02 |
| ± STD Error | 8.56E+05 | 2.39E+05 | 5.61E+04 | 5.00E+03 | 2.17E+03 | 8.48E+02 |
| Dam | Mean | 1.16E+06 | 4.33E+05 | 1.29E+05 | 1.45E+04 | 6.91E+03 | 2.24E+03 |
| ± STD Error | 6.01E+05 | 9.97E+04 | 5.37E+04 | 8.90E+03 | 4.03E+03 | 1.51E+03 |
| Aerosol Extraction Device | Mean | 7.79E+06 | 1.37E+06 | 2.27E+05 | 3.66E+04 | 1.82E+04 | 9.09E+03 |
| ± STD Error | 3.33E+06 | 5.67E+05 | 3.25E+04 | 4.56E+03 | 2.61E+03 | 1.43E+03 |
| Electric Rotor | No mitigation | Mean | 3.49E+05 | 1.63E+05 | 3.96E+03 | 1.10E+03 | 6.50E+02 | 4.26E+02 |
| ± STD Error | 1.45E+05 | 1.33E+05 | 3.96E+03 | 9.88E+02 | 5.83E+02 | 3.94E+02 |
| High-Volume Aspiration | Mean | 0.00E+00 | 0.00E+00 | 0.00E+00 | 3.13E+02 | 3.84E+02 | 3.55E+02 |
| ± STD Error | 0.00E+00 | 0.00E+00 | 0.00E+00 | 3.13E+02 | 3.84E+02 | 3.55E+02 |
| Dam | Mean | 5.80E+05 | 5.58E+04 | 5.64E+02 | 0.00E+00 | 0.00E+00 | 0.00E+00 |
| ± STD Error | 3.55E+05 | 5.58E+04 | 5.64E+02 | 0.00E+00 | 0.00E+00 | 0.00E+00 |

Appendix Table 1: Air particle counts standardized against the baseline data for “Dentist” and “Door” positions for different hand-pieces and mitigation strategies during upper left 2 (UL2) procedures. STD – Standard error of the mean.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |
| UL6 –Dentist & Door |  | 0.3 µm | 0.5 µm | 1.0 µm | 3.0 µm | 5.0 µm | 10.0 µm |
| UL6 - Air - Dentist | No mitigation | Mean | 1.78E+06 | 3.49E+05 | 9.14E+04 | 6.86E+03 | 1.93E+03 | 5.96E+02 |
| ± STD Error | 3.71E+05 | 4.34E+04 | 2.18E+04 | 1.73E+03 | 9.11E+02 | 5.96E+02 |
| High-Volume Aspiration | Mean | 1.89E+05 | 1.43E+04 | 0.00E+00 | 0.00E+00 | 0.00E+00 | 4.41E+02 |
| ± STD Error | 1.10E+05 | 1.30E+04 | 0.00E+00 | 0.00E+00 | 0.00E+00 | 4.41E+02 |
| Dam | Mean | 3.38E+05 | 1.10E+05 | 3.10E+04 | 3.58E+03 | 4.05E+02 | 7.73E+02 |
| ± STD Error | 1.73E+05 | 1.04E+05 | 3.10E+04 | 2.68E+03 | 2.10E+02 | 3.91E+02 |
| UL6 - Air - Door | No mitigation | Mean | 1.25E+06 | 2.65E+05 | 6.59E+04 | 5.89E+03 | 2.47E+03 | 5.79E+02 |
| ± STD Error | 6.13E+05 | 1.08E+05 | 2.52E+04 | 2.11E+03 | 1.14E+03 | 2.01E+02 |
| High-Volume Aspiration | Mean | 1.44E+06 | 2.61E+05 | 2.03E+04 | 3.60E+02 | 8.68E+02 | 3.82E+02 |
| ± STD Error | 1.21E+06 | 2.26E+05 | 1.70E+04 | 3.60E+02 | 8.68E+02 | 3.82E+02 |
| Dam | Mean | 2.63E+05 | 6.88E+04 | 2.24E+04 | 2.27E+03 | 9.64E+02 | 2.80E+02 |
| ± STD Error | 1.46E+05 | 6.88E+04 | 2.24E+04 | 1.84E+03 | 4.94E+02 | 2.80E+02 |

Appendix Table 2: Air particle counts standardized against the baseline data for “Dentist” and “Door” positions for different hand-pieces and mitigation strategies during upper left 6 (UL6) procedures. STD – Standard error of the mean.